**NEW BGZ SERIES – MAXIMAL PERFORMANCE FOR BIG ENGINES**

Une image contenant texte, capture d’écran, batterie

Description générée automatiquement

Une image contenant texte, Appareils électroniques, batterie

Description générée automatiquementUnveiled at EICMA, BS BATTERY has expanded its SLA MAX range with 5 new models called “BGZ Series” to meet the robust performance needs and enduring reliability expected from high-powered touring motorcycles.

These latest AGM generation batteries have been crafted with built-in copper nuts terminal to enhance the conductivity up to 50% than standard terminal and improved max torque strength up to 13N.m. With robust taller plates designed to improve starting power, these 12V batteries offer a maximal performance to big-engine vehicles with high requirements and equipped with lot of electronic equipment’s.

Ready to use, 100% maintenance free and non-spillable, BS BATTERY has unveiled the most powerful models in its Sealed Lead Acid lineup. With a starting power, cycle life and capacity up to 20% higher than the SLA (Sealed Lead Acid) range, the new BGZ series is a premium battery choice for select V-Twin, Metric, ATV and UTV applications!

Discover all BS BATTERY models here:

* [**BGZ 16H**](https://bs-battery.com/product/bgz16h/)
* [**BGZ 16HL**](https://bs-battery.com/product/bgz16hl-sla-max/)
* [**BGZ 20H**](https://bs-battery.com/product/bgz20h-sla-max/)
* [**BGZ 20HL**](https://bs-battery.com/product/bgz20hl-sla-max/)
* [**BGZ 32HL**](https://bs-battery.com/product/bgz32hl-sla-max/)